A B C D E F G H I L M N O P Q R S T U V

## I

I420toNV21Frame(VideoFrame) - function in com.sinch.android.rtc.video.VideoUtils
  Converts frame in I420 to NV21.
INACTIVE - enum entry in com.sinch.android.rtc.calling.CallEndCause
INCOMING - enum entry in com.sinch.android.rtc.calling.CallDirection
initCause(Throwable) - function in kotlin.Throwable
INITIATING - enum entry in com.sinch.android.rtc.calling.CallState
Internals - class in com.sinch.android.rtc
  The following APIs are not considered part of the Sinch SDK stable public API.
isAutomaticAudioRoutingEnabled() - function in com.sinch.android.rtc.AudioController
  Indicates whether the automatic audio routing is enabled.
isBluetoothAudioManaged() - function in com.sinch.android.rtc.AudioController.AudioRoutingConfig
isMute() - function in com.sinch.android.rtc.AudioController
  Indicates whether the microphone is muted.
isSinchPushPayload(Map) - function in com.sinch.android.rtc.SinchPush
  Inspects the payload to decide if it contains Sinch call notification data.
isSpeakerOn() - function in com.sinch.android.rtc.AudioController
  Indicates whether the speaker is enabled.
isStarted() - function in com.sinch.android.rtc.SinchClient
  Indicates if the SinchClient is started.
isTimedOut() - function in com.sinch.android.rtc.calling.CallNotificationResult
  Indicates whether the call has timed out.
isVideoOffered() - function in com.sinch.android.rtc.calling.CallDetails
  Checks whether the caller has offered video.
isVideoOffered() - function in com.sinch.android.rtc.calling.CallNotificationResult
  Returns whether the caller offered video.
isVideoRequested() - function in com.sinch.android.rtc.calling.MediaConstraints
  true if call should contain both video and audio streams, false if only video is requested.

A B C D E F G H I L M N O P Q R S T U V