sinch-rtc

# PushConfiguration

interface PushConfiguration

PushConfiguration specifies configuration needed by the Sinch SDK to initialize managed push functionality allowing clients to receive notifications about incoming calls.

#### See also

HmsPushConfigurationBuilder
FcmPushConfigurationBuilder

## Types

Companion
Link copied to clipboard
object Companion

## Properties

deviceToken
Link copied to clipboard
abstract val deviceToken: String

Device specific token for selected push provider.

vendorData
Link copied to clipboard
abstract val vendorData: Map<String, String>

Optional vendor specific data.

vendorId
Link copied to clipboard
abstract val vendorId: String

Vendor specific id.